INTRODUCTION

In an evolving setting, design interventions need to respond to the specific needs of the users and the constraints associated with the specific site. Designs are generated out of analysis of the relationships between the customary activities of the user and the setting. The GROSSMANN DESIGN GROUP believes that to achieve the optimal design solution, the designer must work intimately with the client and, where ap propriate, the public, to seek design solutions that meet both the client's program and project's budget.

The design methodology focuses on developing technical solutions that meet the client's functional requirements and seeking design solutions within the context of the existing specific project surroundings. This approach to design is particularly applicable to renovation and/or repair projects where the existing facility developments are already in place, and design decisions need to be made within the context of the specific existing facility.

The firm emphasizes careful surveying and investigation of the condition of existing waterproofing membranes and flashings prior to developing recommendations to correct roof deficiencies. Technical recommendations to correct roof deficiencies are developed to meet long term performance requirements.

The GROSSMANN DESIGN GROUP wants the opportunity to prove that a combination of creative design, sensitivity to the environment, and an understanding of project economics and schedule will produce a very successful facility. They invite you to meet with them to discuss together how they can assist you in the development of current and future facili ties.

ROOF REPAIRS AND NEW ROOF SYSTEMS DESIGN FOR FREMONT UNION HIGH SCHOOL DISTRICT • Location • Sunnyvale and Cupertino, California • Size • 5 High Schools • Services • Projects included investigations to evaluate the extent of required roof repairs, and the development of a scope of work and detailed design drawings for the required roofing and flashing repairs. Other projects have included the development of drawings and specifications for new roofing and flashing systems.

ROOF REPAIRS AND NEW ROOF SYSTEMS DESIGN FOR UNITED STATES POSTAL SERVICE FACILITIES, SAN JOSE DISTRICT • Location • Rodeo, St. Rafael, Salinas, Santa Cruz, and San Jose, California • Size • 4,000 - 140,000 SF • Services • Projects included investigations to evaluate the extent of required roof repairs, and the development of a scope of work and detailed design drawings for the required roofing and flashing repairs. Other projects have included the development of technical drawings and specifications for new roofing and flashing systems. Services during construction included providing full-time quality control reviews during the application of the roof membranes and sheet metal flashing assemblies.

TOLMAN HALL RE-ROOFING, McCONE HALL RE-ROOFING AND PENTHOUSE EXTERIOR WALL REPAIRS, A&E BUILDING RE-ROOFING, AND CLARK KERR CAMPUS BUILDING 13 RE-ROOFING • Location • University of California, Berkeley • Size • 5,000 SF - 35,000 SF • Services • The projects have included the development of technical drawings and specifications for new roofing materials. A complete field survey to accurately identify existing conditions was undertaken. Services during construction included providing quality control reviews during the application of the roof membranes and sheet metal flashing assemblies.

FIRE STATIONS, and CORPORATION YARD FACILITIES RE-ROOFING • Location • Sunnyvale, California • Size • 30,000 SF • Services • The project included the development of technical drawings and specifications for new roofing materials. A complete field survey to accurately identify existing conditions was undertaken.

COMMUNITY ACTIVITIES BUILDING ROOF RENOVATIONS • Location • Redwood City, California • Size • 23,500 SF • Services • The project included the development of technical drawings and specifications for new roofing and flashing materials. A complete field survey to accurately identify existing conditions was undertaken.

MUNICIPAL SERVICE CENTER RE-ROOF • Location • Woodland, California • Size • 83,000 SF • Services • The project included the development of technical drawings and specifications for new roofing and flashing materials. A complete field survey to accurately identify existing conditions was undertaken.

SENIOR CENTER ROOF RENOVATIONS • Location • Milpitas, California • Size • 15,800 SF • Services • The project included the development of technical drawings and specifications for new roofing and flashing materials. A complete field survey to accurately identify existing conditions was undertaken.

THE NOB HILL ROOF REPAIRS • Location • San Francisco, California • Size • 6,000 SF • Services • The project included the development of detailed design drawings and specifications for the re-roofing using a high quality roof membrane.

HARBOR HILL EXTERIOR DECK REPAIRS • Location • Tiburon, California • Size • 3 Decks • Services • The project included the development of technical documents for the repair of the exterior decks.

SPYGLASS HILL ROOF REPAIRS • Location • Larkspur, California • Size • 98,000 SF • Services • The project included the development of detailed design drawings and specifications for the re-roofing using a high quality roof membrane.

FAIR OAKS COMMUNITY CENTER ROOF REPAIRS • Location • Redwood City, California • Size • 4,000 SF • Services • The project included the development of detailed design drawings and specifications for retrofitting duct penetrations of the existing roof.

EDGEWATER ISLE SOUTH EXTERIOR DECK REPAIRS • Location • Foster City, California • Size • 60 Decks • Services • The project included the development of detailed design drawings and specifications for the repair of the exterior decks.

2195 GREEN STREET ROOF PATIO RENOVATIONS • Location • San Francisco, California • Size • 1,500 SF • Services • The project included the development of design drawings and technical specifications for a new exterior roof terrace.

BARRON SQUARE DECK REPAIRS • Location • Palo Alto, California • Size • 112 Dwelling Units • Services • The project included an investigation to evaluate the required deck repairs, and the development of detailed design drawings for the required repairs.

ROOF RENOVATIONS FOR THE DIAGNOSTIC SCHOOL FOR THE NEUROLOGICALLY HANDI
CAPPED • Location • Fresno, California • Size • 6,000 SF • Services • The project included an investigation to evaluate the extent of required roof repairs, and the development of detailed design drawings for the required roofing and flashing repairs.

DOLPHIN POINT TOWNHOUSE DECK REPAIRS • Location • Pacifica, California • Size • 9 Dwelling Units • Services • The project included the preparation of design drawings and technical specifications for new balcony waterproofing systems.

COMMUNITY CENTER ROOF RENOVATIONS • Location • Pacifica, California • Size • 22,000 SF • Services • The project included the development of technical drawings and specifications for new roofing materials.

SPORTS CONNECTION/SPECTREM CLUB PARKING DECK WATERPROOFING • Location • San Francisco, California • Size • 48,000 SF • Services • The project included the development of waterproofing systems for the open parking structure located over the health club.

BENIHANA ROOF • Location • Beaverton, Oregon • Size • 6,000 SF • Services • The project included the development of technical specifications for a new clay tile roof and for built-up roofing.

ADMIRALTY DECK REPAIRS • Location • Foster City, California • Size • 80,000 SF • Services • The project included the development of design drawings and specifications for the repair of balcony decks.

SENIOR CENTER RE-ROOFING • Location • Dublin, California • Size • 1,500 SF • Services • The project included the development of technical specifications for new roofing and flashing materials.

2350 EL CAMINO REAL OFFICE TOWER AND CONDOMINIUMS • Location • Mountain View, California • Size • 420,000 SF • Services • The project included the development of technical specifications for new roofing and deck waterproofing materials.

1340 CLAY STREET CONDOMINIUMS • Location • San Francisco, California • Size • 28 Dwelling Units • Services • The project included technical consulting and the preparation of specifications for a building with 28 dwelling units. Special attention was focused on the design of waterproofing systems for the dwelling unit terraces and below grade waterproofing.

SAINT FRANCIS MEDICAL OFFICE BUILDING • Location • San Francisco, California • Size • 60,000 SF • Services • The project included consulting and the preparation of technical specifications for waterproofing of exterior balconies, roof areas above bay windows, and the building roof.

ADDITIONS TO RIVERSIDE COUNTY JUVENILE DETENTION FACILITY • Location • Riverside, California • Size • 10,500 SF • Services • The project included the development of technical specifications for new roofing and flashing materials.

SHEARWATER OFFICE ONE • Location • South San Francisco, California • Size • 380,000 SF • Services • The project included technical consulting and the preparation of specifications for waterproofing systems for the roof and exterior roof terraces.

345 LOCUST STREET RENOVATIONS • Location • San Francisco, California • Size • 11 Dwelling Units • Services • The project included the development of technical specifications for new waterproofing systems for exterior roof terraces and balconies.

SUN TOWER REMODEL • Location • Palo Alto, California • Size • 120,000 SF • Services • The project included the development of technical specifications for the repair of existing roofing and flashing systems.

MISSION SQUARE OFFICE BUILDING • Location • St. Rafael, California • Size • 16,000 SF • Services • The project included the development of technical specifications for a new clay tile roof.

300 THIRD STREET CONDOMINIUMS • Location • San Francisco, California • Size • 220,000 SF • Services • The project included the development of technical specifications for new roofing and flashing materials.

CHERRY BLOSSOM IN SENIOR HOUSING • Location • San Leandro, California • Size • 48,000 SF • Services • The project included the development of technical specifications for new roofing and flashing materials.